Royal Flush

5.10a /Five Card Draw/Emancipation/Mt. Rushmore

Ron Yahne and Jason McNabb 7/30/14

A bolt that was on the previous anchor was over torqued from a previous repair. We pulled this bolt and replaced it with a new triplex bolt. We were able to reuse the Fixe Top Hanger and Quick Link.

**Previous Hardware on Route Repaired:**

Fixe 12mm SS Triplex Bolt (x1)

**BHCC Hardware Installed:**

Fixe 12mm SS Triplex Bolt (x1)